|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| To: RS485  Adapter USB |  |  |  | To: LOR **1**  RS485 In |  |  |  | To: LOR **4** 5V  RS485 In |  |  |
| From: Computer  USB |  |  |  | From: RS585  Adapter Out |  |  |  | From: LOR **1**  RS485 Out |  |  |
|  | To: Computer  USB |  |  | To: RS485  Adapter Out |  |  | To: LOR **1**  RS485 Out |
|  |  |  |  |  |  |  |  |
|  |  | From: RS485  Adapter USB |  |  |  | From: LOR **1**  RS485 In |  |  |  | From: LOR **4** 5V  RS485 In |
| To: LOR **2** In  Tomato Trees |  |  |  | TO: LOR **3** In  Left Yard |  |  |  | To: AlphaPix  DMX Out **1** |  |  |
| From: LOR **4** 5V  RS485 Out |  |  |  | From: LOR **2** Out  Tomato Trees |  |  |  | From: Renard  DMX In |  |  |
|  | To: LOR **4** 5V  RS485 Out |  |  | To: LOR **2** Out  Tomato Trees |  |  | To: Renard  DMX In |
|  |  |  |  |  |  |  |  |
|  |  | From: LOR **2** In  Tomato Trees |  |  |  | From: LOR **3** In  Left Yard |  |  |  | From: AlphaPix  DMX Out **1** |
| To: Renard  DMX Out |  |  |  | To: Router  Port **1** |  |  |  | To: Router  Port **2** |  |  |
| From: Chinese  DMX In |  |  |  | From: Switch  Port **8** |  |  |  | From: Computer  Ethernet |  |  |
|  | To: Chinese  DMX In |  |  | To: Switch  Port **8** |  |  | To: Computer  Ethernet |
|  |  |  |  |  |  |  |  |
|  |  | From: Renard  DMX Out |  |  |  | From: Xmas Router  Port **1** |  |  |  | From: Router  Port **2** |
| To: Router  Port **3** |  |  |  | From: Renard Output **4** |  |  |  | **5** Volts DC  To: LOR **4** |  |  |
| From: AlphaPix  Ethernet |  |  |  | To: Ropes *B V*  Minitrees *R O* |  |  |  | **5** Volts DC  From: Pwr Cntr |  |  |
|  | To: AlphaPix  Ethernet |  |  | **5** Volts DC To: AlphaPix |  |  | **12** Volts DC  To: Chinese DMX |
|  |  |  |  |  |  |  |  |
|  |  | From: Router  Port **3** |  |  |  | **5** Volts DC  From: Pwr Cntr |  |  |  | **12** Volts DC  From: Pwr Cntr |
| **12** Volts DC  To: Amplifier |  |  |  | To: Amplifier  **Left** Out |  |  |  | To: Amplifier  **Right** Out |  |  |
| **12** Volts DC  From: Pwr Cntr |  |  |  | From: Left  Speaker |  |  |  | From: Right  Speaker |  |  |
|  | **12** Volts DC  To: Pwr Cntr |  |  | To: **Left**  Speaker |  |  | To: **Right**  Speaker |
|  |  |  |  |  |  |  |  |
|  |  | **12** Volts DC  From: Amplifier |  |  |  | From: Amplifier  Left Out |  |  |  | From: Amplifier  Right Out |